1.  Introduction

The work described in this report continues similar work described in a previous report [3]. That

report describes a software program that implements an optimal linear demodulator and decoder

for direct-printing radiotelegraph signals commonly used by amateur and commercial stations in

the shortwave radio spectrum. The work described in that report and this one started as an explo-

ration of projects useful in laboratory courses for upper division computer engineering and digital

communications courses; however, both have taken on lives of their own. While laboratory exper-

iments involving audio signal generation and playback are used in existing courses, the limited

processing capability of most available PCs precludes interesting experiments possible with more

sophisticated digital signal processing (DSP) hardware. Since DSP chips have become readily

available and widely used in embedded systems, emphasis is placed on experiments in which

hardware and software designs could be explored in the context of a PC, DSP evaluation board

and a shortwave radio.

This report describes a software program that functions as a radio clock using shortwave radio

signals transmitted by National Institute of Standards and Technology (NIST) radio stations

WWV and WWVH. Operated in conjunction with an inexpensive, fixed-frequency shortwave

radio, it has nominal timing errors less than 125
m
s when tracking one of the stations and fre-

quency variations less than 0.5 parts-per-million (PPM) when not tracking either station. The

clock produces an ASCII timecode that can be used to set the time of another device, such as a

computer, as well as precision reference signals that can be used for other purposes, such as to

drive laboratory test equipment.

The primary reason for choosing the DSP radio clock application is that signal propagation is via

the ionosphere, which acts as an unreliable, multiple reflector, and that the noise process is very

bursty. Thus, the transmission channel model is very much time-varying, sometimes badly dis-

torted by multipath, often contaminated by interfering signals and atmospheric electrical noise,

and sprinkled with dropouts due to strong adjacent channel signals. This presents an interesting

challenge for the student of digital signalling, one unlikely to be found in textbooks. There are

opportunities to devise interesting and insightful approaches to traditional problems such as car-

rier dropout, synchronization recovery, etc., that occur with ionospheric channels.

The primary motivation for this report is as an example and case study of optimum demodulator

and decoder design using a maximum likelihood approach and matched filter, synchronous detec-

tion and soft decision principles. The clock discipline is modeled as a Markov process, with prob-

abilistic state transitions corresponding to a conventional time-of-century clock and the

probabilities of received decimal digits. The result is a performance level which results in very

high accuracy and reliability, even under conditions when the one-minute beep from the WWV/H

signal, normally its most prominent feature, cannot be detected by ear with a sensitive communi-

cations receiver.

This report proceeds first with a discussion on the design approach followed by a description of

the WWV/H transmission format and an overview of the hardware architecture. The detailed

design of the DSP clock is described by each functional block. This includes the processing steps

at the radio frequency and baseband stages of processing. The discussion proceeds with a detailed

mathematical analysis of performance and ends with an evaluation of performance under real

world conditions. Appendix A contains operation notes, including status indicators, command
functions and signal inputs and outputs.

2.  Design Approach

The DSP clock is designed for use with an inexpensive shortwave radio, although for testing it has
been used with a sensitive communications receiver and laboratory equipment, including a signal
generator, oscilloscope and calibrated cesium clock. It is intended to work with indoor antennas in
most cases, although for testing an elaborate outdoor antenna has been used. The radio IF band-
width and stability are ordinarily not a factor, since the emissions are amplitude modulated and
the DSP-93 program includes all necessary signal conditioning and bandwidth filtering. Most
shortwave radios today have high sensitivity for use with telescoping rod antennas. However,
shortwave stations normally operate with hundreds of kilowatts and highly directional antennas,
while the WWV/H stations operate with only 10 kW and nondirectional antennas. In most situa-
tions, something more than a telescoping rod, perhaps a hank of wire strung across the ceiling or
tossed out a window may bring better results.

Shortwave transmissions are propagated via single or multiple reflections between the ionosphere
and the ground. The path geometry depends on up to three ionospheric layers, which vary in
height over the days, seasons and years. One result is the best frequency to use at any hour of the
day depends on the height of these layers and the intensity of solar radiation over the ray path.

Usually, the higher frequencies work best during the day and the lower at night. Commercial radio
clocks that use WWV/H signals, such as the GC-1000 Most Accurate Clock, originally marketed
by the Heath Company, and the 1020 Time Source, originally marketed by Precision Standard

Time International, use frequency-agile receivers that automatically tune the embedded receiver to
the frequency with the strongest signal.

However, to avoid complexity and cost, the DSP clock is designed to operate on only one fre-
quency. The best frequency to use depends on the distance from the transmitter and must be cho-
sen by compromise. Usually, the lower frequencies are better nearer to the transmitter and the
higher frequencies are better further away. When more than one frequency is usable, it is usually
best to chose the higher one. In some cases it may be best to choose a compromise frequency that
works best near sunrise and sundown. In any case, the best choice depends on location, ambient
noise level and antenna configuration.

In order to succeed in this approach the DSP clock must have the highest sensitivity and reliability
when only marginal signals are available. This is the main reason so much emphasis has been
placed in sensitivity and reliability under adverse conditions. In extreme cases, it may be possible
to synchronize the clock only near sunrise and sunset and, even then, maybe not every day. A crit-
ical consideration in this regard is the frequency variations of the DSP chip clock oscillator due to
ambient temperature variations. With the current hardware and ordinary room temperature varia-
tions, this limits the accuracy to the order of a millisecond per hour when the radio signals are not
available.

3.  WWV/H Signal Design

The DSP clock uses signals transmitted by frequency and time stations WWV, located in Ft. Col-
lins, CO, and WWVH, located in Kaui, HI. Both stations transmit amplitude-modulated signals

on standard frequencies of 2.5, 5, 10 and 15 MHz (WWV includes 20 MHz) using a program of

voice announcements and audio tones at 440, 500 and 600 Hz. In addition, the stations transmit a

time-of-century digital timecode designed for displays and other electronic media. Only the time-

code and related pulses at 100, 1000 and 1200 Hz are used by the DSP clock.

The WWV signal format is described in [5]. It consists of three elements, a 5-ms, 1000-Hz pulse,

which occurs at the beginning of each second, a 800-ms, 1000-Hz pulse, which occurs at the

beginning of each minute, and a pulse-width modulated 100-Hz subcarrier, which carries the data

bits. The WWVH format is identical, except that the 1000-Hz pulses are sent at 1200 Hz. The sec-

ond and minute pulses are transmitted at 100-percent modulation, while the subcarrier modulation

is transmitted 10 dB below the 100-percent level, one pulse per second. In the Inter-Range Instru-

mentation Group (IRIG) code, from which the WWV/H code is derived, a zero is encoded as a

200-ms pulse, one as a 500-ms pulse and a special position marker as a 800-ms pulse. However, in

the WWV/H format, the subcarrier is suppressed for the first 30 ms of the second, in order to

make room for the 5-ms sync pulse.

Each minute encodes nine BCD digits for the time plus seven miscellaneous bits, as shown in Fig-

ure 1. There is no subcarrier modulation in second zero of the minute, in order to make room for

the 800-ms sync pulse. Also, second 60 is present only on the occasion of a leap second. There are

six position identifiers, encoded P1 through P6, which are intended to assist the synchronization

and decoding functions in some equipment, but are not used by the DSP clock. Seconds not num-

bered in the figure are not used in the current transmission format and are sent as zeros.

The time-of-century is sent as nine BCD-encoded digits, low-order bit and least-significant digit

first. The leap warning bit indicates that a leap second is to be inserted after the last minute of the

last day of June or December and is numbered second 60 of that minute. The DST1 bit is set to

                                          Sec Sec Sec Sec

                                                  0 no carrier 15 minute 10 30 day 1 45

                                                  1 DST2 16 minute 20 31 day 2 46

                                                  2 leap warning 17 minute 40 32 day 4 47

                                                  3 18 33 day 8 48

                                                  4 year 1 19 P2 34 49 P5

                                                  5 year 2 20 hour 1 35 day 10 50 DUT sign

                                                  6 year 4 21 hour 2 36 day 20 51 year 10

                                                  7 year 8 22 hour 4 37 day 40 52 year 20

                                                  8 23 hour 8 38 day 80 53 year 40

                                                  9 P1 24 39 P4 54 year 80

                                              10 minute 1 25 hour 10 40 day 100 55 DST1

                                              11 minute 2 26 hour 20 41 day 200 56 DUT .1

                                              12 minute 4 27 42 57 DUT .2

                                              13 minute 8 28 43 58 DUT .4

                                              14 29 P3 44 59 P6

60 leap second

Figure 1. WWV/H Timecode For mat

one at 0h UTC on the day of transition to daylight time and thereafter and set to zero at 0h UTC
on the day of transition to standard time and thereafter. The DST2 bit follows the state of the

DST1 bit, but delayed 24 hours later. The DUT sign and magnitude encode the UT1 time correc-
tion in tenths of a second. The UT1 correction is used by astronomers and navigators to establish
a precise star transit time.

4.  Hardware Functional Description

The hardware chosen for the DSP clock is called the DSP-93 and is supplied in kit form by the
nonprofit Tucson Amateur Packet Radio (TAPR) organization operating in partnership with the

Amateur Satellite (AMSAT) organization. Previously, TAPR developed the packet radio technol-
ogy commonly used by for-profit firms manufacturing inexpensive VHF and UHF wireless
modems. The DSP-93 includes a Texas Instruments (TI) TMS320C25 DSP chip [6] and various
interface chips for analog/digital conversion, radio control and serial input/output interface to the

PC. The TMS320C25 uses a 16-bit pipelined design and operates with a 40-MHz clock and 10

MIPS instruction rate. It communicates with the PC using a universal asynchronous receiver/
transmitter (UART) chip operating at 19,200 baud.

The DSP-93 consists of a digital circuit board, an analog circuit board and an external power sup-
ply transformer. The digital board includes the TMS320C25, 256K words of EPROM used for the
monitor program, 32K words of program RAM and 32K words of data RAM. The monitor pro-
gram is used only during program development. The analog board includes a TI TLC32044 14-bit
voiceband analog interface chip [7], a 16550 UART and various chips for audio processing and
transceiver control.

Figure 2 is a block diagram of the DSP-93 hardware components. The DSP-93 program controls
the front panel LED display, the UART used to communicate with the PC program, the analog/
digital converter (ADC) and digital/analog converter (DAC) in the analog interface, as well as two
audio switches and the transceiver control interface. One of the audio switches selects which of
several sources are input to the ADC, including the Audio In input of either transceiver port, the

DAC output for test signal generation and monitoring, or the auxiliary (Squelch) input of either
transceiver port. The other audio switch is used in the feedback path of a differential amplifier to
implement a programmable gain function. Potentiometers are provided to set audio input and out-
put levels for each transceiver port.

The DSP-93 program can individually control either of two transceivers, one connected to each
radio port, using the push-to-talk (PTT) output, which serves the same function as on a typical
mobile microphone. Most transceivers can connect the Audio Out directly to the microphone
audio input; however, some transceivers equipped for direct FSK keying can use the Key output
instead. Some transceivers are equipped to shift operating frequency in discrete steps up or down
in response to a button press on the microphone. The program can use the Freq Up and Freq Down
outputs to perform these same functions.

The analog interface includes, besides the basic ADC and DAC functions, a set of programmable
dividers driven from the TMS320C25 clock. As used by the DSP-93 program, these dividers are
programmed to provide a basic analog/digital conversion clock rate as close to 8000 Hz as possi-
ble. This clock rate was chosen both for compatibility with standard telephone conventions, as
well as a compromise between various sources of noise and available processing latencies.

The monitor program resides in EPROM on the digital board. It includes a rudimentary debugger,

program loader, a suite of prebuilt modem programs, and a set of utility programs, including a

digital oscilloscope and spectrum analyzer. The program loader is used to load DSP-93 programs

developed on the PC, but is disabled when the DSP-93 program is in operation. Current program

development tools include a rudimentary shareware assembler, which is quite adequate for this

application.

5.  Software Functional Description

The DSP-93 program consists of interlocking loops driven by hardware interrupts from the ADC,

DAC and UART. At the heart of the program is a circular buffer which holds input samples from

the ADC before processing by the program and output samples from the program before output to

the DAC. The buffering strategy, adapted from [3], is designed to relieve the programmer from

intricate loop unrolling and decimating. Most of the interrupt, buffering, command interpretation

and storage management functions were incorporated intact from the high performance modem

program described in [3] and will not be described further here.

LEDs UART EPROM

RAM

TMS320

Transceiver

Control

(2 ports)

Key

PTT

Freq Up

Freq Down

Squelch

Audio In

Audio Out

DAC

ADC

Source

Switch

                                                                            Gain

                                                                     Switch

Amp

Host Computer

External

Bus

Figure 2. DSP-93 Hardware Architecture

5.1  RF Filtering and Sync Extraction

A block diagram of the DSP processing is shown in Figure 3. The analog audio signal from the
radio is sampled at 8000 Hz and converted to digital representation. The 1000/1200-Hz pulses and

100-Hz subcarrier are first separated using two FIR filters, a 400-Hz bandpass filter centered on

1100 Hz and a 150-Hz lowpass filter. Figure 4 shows the response of the bandpass filter, while

RF
filter
phase-lock
oscillator

1-s
sync

1-m
sync
sample
clock

1000 Hz

100 Hz

seconds
counter
envelope
demodulate

noise
estimate
decoding matrix
digit correlator

clock counter
minutes of century

                                                                  ADC

Figure 3. DSP Clock Software Architecture

Q channel

I channel

          In

Figure 4. 400-Hz Bandpass Filter Response

Figure 4 shows the response of the lowpass filter. As evident on both figures, the stopband attenu-

ation is at least 40 dB.

The 1-s sync pulse is extracted using a 5-ms matched filter and exponentially averaged in a comb

filter. Figure 5 shows the output of the WWV matched filter with the 5-cycle WWV signal, while

Figure 6 shows the output of the same filter with the 6-cycle WWVH signal. The plots show a 6-

dB difference in the peak amplitude, which is the only way the DSP clock can differentiate

between the two stations. The maximum over all 8000 stages of the comb filter establishes the

first sample of the second. The 1-m sync pulse is extracted using a 800-ms noncoherent integrator

and exponentially averaged in a comb filter. The maximum over all 60-stages of the comb filter

establishes the first second of the minute.

Figure 4. 150-Hz Lowpass Filter Response

Figure 5. 1-s Matched Filter Output - WWV Signal

4. The pulse length must be in the range 200-1000 ms.

If any of these sanity checks fail, the data bit is considered invalid and all three probabilities are
set to zero.

The difference between the P1 and P0 probabilities for each data bit is exponentially averaged in a
set of 60 accumulators, one for each second, to determine the semi-static timecode data, such as

DST indicator, leap second warning and DUT correction. In this design, an average value larger
than a positive threshold (+1000) indicates as one and a less than a negative threshold (
-

1000) as
zero. Values between the two thresholds, which can occur due to signal fades or loss of signal, are
interpreted as ^don´t care,~ and result in no change of indication.

The sanity checks and decision thresholds have been established experimentally for reliable sub-
carrier demodulation, while the probability mappings have been chosen for reliable pulse-width
demodulation of the data signal itself. Correct PLO phase is also essential for reliable data recov-
ery. The principal hazards in this process are phase discontinuities during times the WWV/H sig-
nals are rising from the noise to useful levels and, especially, when signals from both WWV and

WWVH are received at the same time and interfere with each other due to different ionospheric
ray paths.

5.3  Digit Decoding

The BCD digit in each digit position of the timecode is represented as four data bits, all of which
must be valid for the digit itself to be considered valid. If so, the bits are correlated with the bits
corresponding to each of the valid decimal digits in this position. If the digit is invalid, the corre-
lated value for all digits in this position is assumed zero. In either case, the values for all digits are
exponentially averaged in a likelihood vector associated with this position. The digit associated
with the maximum over all of the averaged values then becomes the maximum likelihood selec-
tion for this position.

The decoding matrix contains nine row vectors, one for each timecode digit position. Each row
vector includes the likelihood vector, along with other related data. The maximum likelihood digit
for each of the nine digit positions becomes the maximum likelihood time of the century. A built-
in transition function implements a conventional clock with decimal digits that count the minutes,
hours, days and years, as corrected for leap seconds and leap years. The counting operation also
rotates the likelihood vector corresponding to each decimal digit as it advances. Thus, once the
seconds and minutes have been synchronized, the maximum likelihood time in any minute should
correspond to the BCD timecode transmitted in that minute.

Each row of the decoding matrix includes the likelihood vector, clock digit, a compare counter
and the difference (mod 10) between the current clock digit and most recently determined maxi-
mum likelihood digit. If a digit probability exceeds the decision level and the difference is con-
stant for four successive minutes in any row, the maximum likelihood digit replaces the clock digit
in that row. When the differences are zero for all rows, the clock is synchronized and delivers cor-
rect time to the integral second. The millisecond within the second is derived from the ADC sam-
ple clock, which runs at 8000 Hz and drives all system timing functions.

In addition to the synchronization indicator character in the ASCII timecode, four status bits are
encoded in a quality character. One bit indicates whether the seconds and minutes are synchro-

nized, another indicates whether any of the likelihood values are less than the decision threshold,

a third indicates whether the subcarrier envelope for any second is valid, and the fourth indicates

whether any maximum likelihood digit differs from the corresponding clock digit. In addition, a

set of control commands can be used to select the operating mode and optional debug message

types.

An important feature of the DSP clock design is that the maximum likelihood digit depends only

on the correlated digit values, which are exponentially averaged. Valid new data in effect charges

the likelihood values, while the absence of new data slowly discharges them. Since the maximum

likelihood digit depends only on comparing likelihood vector entries and the integration constant

for all entries is the same, the digit is unchanged even under propagation conditions which result

in missing timecode bits or BCD digits. If under these conditions the maximum likelihood value

for any digit decays below the decision threshold, the compare counter is reset and updating of

that digit is suspended.

6.  Performance Analysis

Since the DSP clock operates under conditions where received WWV/H signals normally vary

from unusable to excellent, the DSP-93 program design places considerable emphasis on avoiding

false indications due to marginal data and destructive interference between WWV and WWVH

signals when both are received at the same time. A successful synchronization sequence requires

each of a series of steps to be completed before the next step is begun and all steps must be com-

pleted before any changes are made to the clock digits or miscellaneous bits. This section dis-

cusses the performance of the DSP clock with respect to signal to noise ratios and error rates for

the synchronization, demodulation and decoding functions.

In the following, the signal to noise ratio (SNR) is defined as symbol energy divided by noise

power density E

                                                                                                               s

                                                                                                                    / N

0

, where the noise process is assumed Gaussian. The general plan is to first

derive the processing gain, defined as the SNR improvement between the input and output of the

various filtering and averaging algorithms, then establish the required SNR for specified error

rate, and finally compute the minimum acceptable SNR at the DSP-93 audio input.

The first step is second synchronization recovery. From standard analysis [1], the 400-Hz band-

pass filter and 5-ms matched filter provide an SNR improvement of 10log(2 T

s

B ), where

B = 2100 Hz is the input bandwidth and T

s

= 5 ms is the integration time, or 10.2 dB. It is neces-

sary to distinguish the center cycle of the matched filter signal from the eight others that accom-

pany it; but as shown in Figure 5, this cycle has amplitude only 1/5 more than the two surrounding

it, which results in a processing loss of 7 dB and a total processing gain of 10.2

-
7 = 3.2 dB. The

averaging constant of the 1-s comb filter follows the frequency averaging interval at 1/4 its value.

At the longest interval, the averaging constant is 256, which results in a processing gain of

10log(256) = 24.1 dB and a total processing gain of 3.2 + 24.1 = 27.3 dB.

If P

                          e

                                 is the probability of a single error (wrong choice of center cycle), then P

e

(1

-
P

e

)
n

 is the

probability of a run of n  samples ending in an error. If half of these runs have ten samples or more,

then P

                                          e

                                                 must be less than .075. This is a conservative bound, since the median filter corrects a sin-

gle error. Selection of the center sample amounts to detection of an on-off keyed (OOK) wave-

form, which has bit error rate  [1]. For the assumed

P

         e

                   = .075, the SNR must be greater than 3.2 dB. Since the 1-s sync pulse is transmitted at 100 per-
cent carrier modulation, which is 3 dB below the carrier power, the minimum SNR at P
e

= .075 is

3 + 3.2
                                               -

                                                        27.3 =
                                                                                                       -

                                                                                                                21.1 dB. At this SNR, it is very unlikely that the 1-s sync pulse can be detected
by ear, even with a sensitive communication receiver.

Once the second has been synchronized, the 100-Hz PLO operates continuously to establish the
correct subcarrier phase, as described above. The processing gain for the PLO demodulation using
matched filters is 10log(2 T
s

B ), where B = 2100 Hz and Ts = 170 ms, or 25.5 dB. Invoking the
same argument as for the 1-s sync signal, but accounting for the subcarrier modulation 10 dB
below 100 percent, the minimum SNR at P
e

= .075 is 13 + 3.2
-

25.5 =
-

9.3 dB. Note that the dis-
tinction between a P0 and P1 pulse is equivalent to detecting an OOK pulse occupying the interval

200-500 ms in the second. The 170-ms matched filter is suboptimal for this, but not enough to sig-
nificantly affect the conclusions.

The next step is minute synchronization recovery. The noncoherent integrator sums the I-channel
and Q-channel squares for 800 ms in the first second of the minute. The processing gain is

10log(800/2) = 26 dB. The 1-m comb filter has an averaging constant of 8, which provides an
additional processing gain of 10log(8) = 9 dB, for a total of 35 dB. Again invoking the analysis
used for the 1-s sync pulse, the minimum SNR at P
e

= .075 is 3 + 3.2
-

35 =
-

28.8 dB. At this
level, it is very unlikely that the 1-m sync pulse can be detected by ear. even with a sensitive com-
munication receiver.

Once the minute has been synchronized, miscellaneous timecode bits are demodulated and expo-
nentially averaged as described above. The bit error rate, even at P
e

= .075, is very low due to the
hysteresis thresholds at ±1000 and the averaging constant of 16, which is equivalent to a time con-
stant of 16 minutes. In effect, this adds another 12 dB to the processing gain and results in a mini-
mum SNR at P

                                                                                                   e

                                                                                                             = .075 of
-

9.3
-

12 =
-

21.3 dB. Note that the minimum SNR for both second and
minute synchronization are well below the minimum SNR for subcarrier demodulation, so that in
the demodulation analysis the effects of synchronization errors can be neglected.

The next step is to determine the digit in the minute units digit position. This must be done before
any other digit in the timecode, since only when the carry from the minute units digit has been
determined can the higher order carries be determined. When four minute digits with maximum
likelihood values exceeding a decision threshold of 1000 have been successfully compared, the
minute units clock digit is set and the remaining likelihood vectors allowed to accumulate values.

No matter what the phase of the remaining digits happen to be, there is at least ten minutes to
accumulate values before any of these digits can change. Normally, this is sufficient time for the
likelihood values to rise above the decision threshold and the compare process to begin.

To set a clock digit, a run of four, 4-bit BCD digits must be correctly decoded. The probability that
a run of 16 or more correct bits will occur at least half the time requires P
e

 less than .045, which in
turn requires a minimum SNR of 4.5 dB. But, the likelihood values are integrated with an averag-
ing constant of 16, which provides a processing gain of 12 dB. Together with the subcarrier pro-
cessing gain derived above, this results in a minimum SNR of 4.5
-

9.3
-

12 =
-

16.2 dB.

P
e

Q E
s

N

0

¤

( )

1

2

-

-

- erfc sqrt

S N R

2

-

-

--

-

--

-

-

-

-
è ø

æ ö
è ø

æ ö

= =

The clock can be set wrong only if four or more successive maximum likelihood digits are wrong.

The probability of a digit decoding error at the P

e

=.045 is 1

-
(1

-
P

e

)

4

= 0.169. A clock error will

occur if four or more such decoding errors occur in a row, which occurs with probability 9.8x10

-4

,

or about 1.4 errors per day. It is important to note that such periods when operating at the mini-

mum SNR assumed here are short, generally lasting only a few minutes as propagation conditions

open and close between WWV/H and the radio location. At other times, either the signal is com-

pletely absent or well above the minimum SNR.

7.  Measured Performance

An important goal in the DSP clock design is that the accuracy and stability of the indicated time

be limited only by the characteristics of the propagation medium. Conventional wisdom is that

time synchronization via the shortwave medium is good only to a millisecond under the best prop-

agation conditions. The performance of the DSP clock tracking the WWV/H signals is clearly bet-

ter than this, even under marginal conditions. Ordinarily, with marginal to good signals and a

frequency averaging interval of 1024 s, the frequency is stabilized within 0.1 PPM and the time

within 125

                                                                           m
                                                                                     s. The frequency stability characteristic is highly important, since the clock may have

to free-run for several hours when the WWV/H signals are unavailable.

The time accuracy over a typical day has been measured using an oscilloscope and cesium oscilla-

tor calibrated with a GPS timing receiver. With marginal signals and allowing 15 minutes for ini-

tial synchronization and frequency correction, the time accuracy determined from the 1-s sync

pulse is reliably within 125
m
s. In the particular DSP-93 used for program development, the

uncorrected clock frequency offset is 45.8±0.1 PPM. Over the first hour after initial synchroniza-

tion, the clock frequency varies about 1 PPM as the frequency averaging interval increases to the

maximum 1024 s.

Figures 8 through 13 show the DSP clock behavior measured under typical conditions over three

days and nights in late July, 1997. For these tests the radio was a sensitive communications

receiver and the antenna a 135-foot dipole 12 meters above the ground. The tests were designed to

establish SNR margins that might be expected using less dramatic radios and antennas. Reception

during daylight hours was generally good, with signals ranging from S3 to S9, as measured by the

communications receiver signal strength meter. The data from which the figures were made were

collected in real time by the running DSP-93 program and saved in a file on a Unix workstation.

These files were later processed using the Math Works MatLab [4] and the Signal Processing

Toolbox [2] to produce the figures themselves.

At the time of year the tests were performed, the propagation path between the WWV transmitter

at Boulder, CO, and the radio at Newark, DE, is open from middle morning to late evening in

Newark. Figure 8 shows the 1-s sync pulse amplitude during the measurement period in decibels.

The ratio of the maximum daytime amplitude to the maximum nighttime amplitude represents an

SNR of about 40 dB during the daytime. The 1-s sync decision threshold is set at 1500, which cor-

responds to 63.5 dB on the plot. The SNR margin is defined as the excess SNR over the decision

threshold, in this case about 17 dB during the daytime. With another radio and antenna, the perfor-

mance relative to the test setup could be up to 17 dB worse and still successfully synchronize the

second. However, the decision threshold is itself set about 24 dB above the noise floor, far above

the required minimum SNR of 3.2 dB, and could probably be reduced without increasing the
false-alarm rate. Note that, near sunrise and sunset at the midpoint of the path, it is not uncom-
mon for the signal to fade in and out and, while not evident from the figure, for both WWV and

WWVH stations to be heard at the same time. These are the occasions of maximum stress on
the engineered algorithms to avoid false indications.

Figure 9 shows the 1-m sync pulse amplitude in decibels. While the ratio of the maximum day-
time amplitude to the maximum nighttime amplitude represents an SNR well over 60 dB, this
figure is misleading, since the 1-m signal is enabled only if the 1-s signal has successfully syn-
chronized the second. The 1-m sync decision threshold is set at 500, which corresponds to 54
dB on the plot and an SNR margin of about 26 dB. As in the 1-s sync pulse case, the threshold
could probably be reduced without increasing the false-alarm rate. The plot shows the results of

Figure 8. 1-s Sync Pulse Amplitude

Figure 9. 1-m Sync Pulse Amplitude

almost 16 s of integration and suggests that minute synchronization may never be a problem, even

on far weaker signals.

Figure 10 shows the 100-Hz subcarrier SNR, measured as the ratio of the peak I-channel level to

the average Q-channel level in decibels. The ratio of the maximum daytime amplitude to the max-

imum nighttime amplitude represents an SNR of about 25 dB during the daytime. The SNR deci-

sion threshold is set at 8, which corresponds to 18.1 dB, and an SNR margin of about 12 dB. As

the only function of this threshold is to confirm that the subcarrier phase is in the correct quadrant,

it could probably be reduced by a few decibels without increasing the false-alarm rate. While a

margin of 18.1 dB is somewhat less than the other margins, there is still much more processing

gain before a digit is decoded or a miscellaneous bit is set. One thing to note about the plot is the

very wide variation over almost 40 dB during the day As as the signals fade in and out.

Figure 11 shows the likelihood values in decibels. While the ratio of the maximum daytime ampli-

tude to the maximum nighttime amplitude represents an SNR well over 60 dB, this figure is mis-

leading, since only valid data bits are considered for likelihood and correlation computations. The

likelihood decision threshold is set at 1000, which corresponds to 60 dB on the plot or an SNR

margin of about 17 dB. As in the other cases, this threshold could probably be reduced without

increasing the false-alarm rate.

With the above data in hand, it is possible to predict how the DSP clock would function with

weaker signals than observed during the measurement period. Informal observations confirm that

the WWV/H signals produce reliable indications, even when the voice announcements and audio

tones cannot be heard. The data show a 1-s sync pulse margin of 17 dB, a 1-m sync pulse margin

of 26 dB, a subcarrier SNR margin of 12 dB and a likelihood margin of 17 dB. Clearly, the factor

limiting sensitivity is the subcarrier SNR threshold. As mentioned earlier, the SNR threshold

could probably be reduced by a few decibels without increasing the error rate, which would raise

the overall DSP clock margin to 17 dB. The subcarrier PLO design has not been optimized and the

SNR determination is rather crude. However, the present design performs far better than the best

Figure 10. 100-Hz Subcarr ier SNR

known commercial radio clocks, so it may not be worthwhile to squeeze out the last ounce of pro-
cessing.

Figure 12 shows the clock oscillator frequency variations over the period. During intervals when

WWV/H signals are available, the trace varies over almost 1 PPM, but at other times appears as a
straight line. It is not clear whether the variations are due to doppler as the ionospheric layers rise
and fall, to the inherent instability of the DSP-93 clock oscillator, or some combination of both.

The characteristics shown in the figure suggest that much of the variation may be due to iono-
spheric motion. To the extent that this motion cannot be reliably predicted and the frequency var-
ies typically over 0.5 PPM, a phase adjustment as high as 18 ms may be necessary after ten hours
with no signal. Figure 13 clearly shows these phase adjustments as discontinuities when the

WWV/H signals resume after some hours when they are unavailable.

Figure 11. Digit Likelihood Values

Figure 12. Clock Oscillator Frequency

The propagation delay from the WWV transmitter at Boulder, CO, to a communications receiver

and DSP clock at Newark, DE, is 23.5±0.1 ms, as measured by a calibrated cesium clock. The

delay is measured to the peak of the pulse after the 1-s sync comb filter and includes components

due to the ionospheric propagation delay, receiver delay and DSP-93 delay. The measured DSP-93

delay is 5.5 ms, most of which is due to the 400-Hz bandpass filter and 5-ms matched filter.

8.  Conclusions

It is tempting to consider the ultimate DSP clock performance capability. The most critical limit-

ing factor in performance is the PLO, which is necessary only because the phase delay character-

istics of the particular radio are not known and must be measured during operation. It should be

noted that the DSP-93 clock frequency depends only on the 1-s sync pulse and the PLO is used

only to adjust the phase. The subcarrier SNR decision threshold is used only to confirm the PLO

has indeed locked on the correct phase. Thus, a simple solution would be to reduce the PLO loop

gain, effectively increasing the time constant. This would require a better DSP-93 clock oscillator

such as a TCXO. Once reliable phase has been determined, which may take some time, the PLO

feedback loop can be opened, the SNR gate removed and the 100-Hz signal left on dead reckon-

ing.

Once the subcarrier SNR threshold has been removed, the likelihood margin of 17 dB becomes a

limiting factor. As long as correct second and minute synchronization can be maintained, the inte-

gration time, currently 16 m, can be increased indefinitely. As a practical matter, an increase of

four times (6 dB) coupled with reducing the likelihood threshold by 3 dB would raise the margin

to 26 dB. At this point, the 1-s sync margin would be the limiting factor. Increasing the integration

time by 6 dB plus lowering the threshold by 3 dB would raise the margin to 26 dB, making the

overall margin for the DSP clock to 26 dB. This might even allow a paperclip to be used as an

antenna or, with a good antenna, a reduction in WWV/H transmitter power from 10 kW to a

pipsqueak 25 W.

Figure 13. Clock Phase Adjustments

LED4 Sync indicator. Blinks to indicate 1-s and 1-m sync. Short blinks follow the 1-s sync pulse,

                                                  while long blinks follow the 1-m sync pulse. This is active when in 1-s sync and indefi-

                                                  nitely after the clock has been synchronized. If the clock has not been in both 1-s sync and

                                                  1-m sync during the minute, status bit 0 is set in the following minute.

LED5 Data present. On for one second only when in 1-s sync and following a data bit with

                                                  amplitude above the decision threshold. A data bit with amplitude below the decision

                                                  threshold has assumed bit probability of zero, but does not necessarily indicate a clock

                                                  error. Note that there is no data bit in second zero of the minute. If LED5 has not been on

                                                  during the minute, status bit 1 is set in the following minute.

LED6 Low decoded signal probability. On only in 1-s sync and when a correlated bit or digit

                                                  probability is below the decision threshold. The associated bit probability is zero, but does

                                                  not necessarily indicate a clock error. LED6 when on causes status bit 2 to be set in the fol-

                                                  lowing minute.

LED7 Decoding error. On only in 1-s sync and when the maximum likelihood digit differs from

                                                  the current clock digit. The associated digit is not used to set the clock, but does not neces-

                                                  sarily indicate a clock error. LED7 when on causes status bit 3 to be set in the following

                                                  minute.

LED8 DSP-93 Power indicator

10.2  Program Commands

The DSP-93 program responds to a number of commands, which consist of a single case-insensi-
tive letter followed in some cases by one or more digits. Control characters, including CR and LF,
are ignored, except in the C and H commands. The station to be monitored is selected using the C

(WWV) or H (WWVH) commands. The only affect these commands have is to select which 5-ms
matched filter to use for the 1-s sync, which tone (1000 Hz or 1200 Hz) to use for the 1-m sync
integrator, and which propagation delay value to use. These commands can be followed by a deci-
mal number, which specifies the propagation delay in 125-us units, and then a CR to enter the
value. A C or H command followed immediately by a CR selects the station, but does not change
the propagation delay.

B{0-9}

This command selects the UART baud rate. The digit argument is interpreted as follows:

0 300

1 600

2 1200

3 2400

4 4800

5 9600

6 19200

7 38400

8 76800

9 153600

The default is set by the program loader, which is 19200 with the TAPR firmware monitor.

P{0-2}

This command enables or disables either the RTS or DTR line from the UART to follow LED4.

Note that internally the UART RTS output is connected to the CTS pin (8) on the DB9 connector.

The digit argument is interpreted as follows:

0 RTS and DTR always high

1 RTS follows LED4, DTR always high

2 DTR follows LED4, RTS always high

R

This command resets the DSP clock to the initial state at the point control is transferred by the

TAPR firmware monitor to the DSP-93 program.

S{0-9}

This command sets the nine digits of the clock from low to high order. This command is useful in

order to verify proper rollover of the leap second and leap year, for example.

T

This command returns the timecode string in the following format preceded by a CR/LF

sequence. This format conforms to Format 2 as used by the Spectracom WWVB and GPS radio

clocks and supported by the current version of the Network Time Protocol (NTP) software for

Unix and Windows.

sqyy ddd hh:mm:ss.fff ld

s sync indicator (`?´ or ` `)

q quality character (` `)

yy year of century

ddd day of year

hh hour of day

mm minute of hour

ss second of minute

fff millisecond of second

l leap second warning ` ` or `Ĺ

d DST state `S´, `D´, `I´, or `O´

The on-time reference is the start bit of the first (CR) character. The sync indicator s is `?´ until the

clock is set by valid received data and ` ` after that. The quality character q is always ` ` in this for-

mat.

The leap second warning l is `Ĺ if a leap second is expected at the end of the month and ` ` if not.

By international agreement, the leap second is inserted following the last minute of the last day of

June or December and is numbered second 60 of that minute. The WWV/H timecode progression

just before, during and after the leap on 30 June 1997 is shown below, where the first column is

the year, followed by the day, time, leap second warning, DST state and DUT correction (see U

command):

97 181 23:59:59 LD -5

97 181 23:59:60 LD -5

97 182 00:00:00 D +5

Note the seconds progression includes second 60 of the last minute and the day number advances
at the next second. Also, the leap warning disappears and the DUT correction -5 changes to +5 at
that time; however, in actual use these changes are delayed a few minutes as the result of the inte-
gration functions.

The DST state is determined from the DST1 and DST2 bits of the WWV/H timecode. The DST1
bit is set to one at 0h UTC on the day of transition to daylight time and thereafter. The bit is set to
zero at 0h UTC on the day of transition to standard time and thereafter. The DST2 bit bit follows
the state of the DST1 bit, but delayed 24 hours later. The values are decoded as follows:

S standard time

D daylight time

I between 0h on the day to daylight time until 0h the next day

O between 0h on the day to standard time until 0h the next day

U

This command returns the timecode string in the following format followed by a CR/LF sequence.

This format is intended for experimentation and evaluation and may be changed in future.

sq a yy ddd hh:mm:ss.fff ld dut ttttt fffff ggggg uuuuu
where the elements of the timecode are as described for the T command, with the addition of the
following:

q quality character_a station select C (WWV) or H (WWVH)
dut DUT sign and magnitude in deciseconds
ttttt median filter time offset in 125-us units
fffff frequency offset in units of about 1.9 ns/s
ggggg frequency averaging interval in seconds_uuuuu interval since last clock update in minutes

The on-time reference is the start bit of the first (s) character.

The quality character encodes four bits of status formatted in hex. Reading from high to low order,
the bits are:

0 low 1-s or 1-m sync pulse amplitude

1 low 100-Hz subcarrier amplitude

2 low decoded digit probability_3 timecode digit decoding error

The DUT sign and magnitude encode the UT1 time correction in tenths of a second. The UT1 cor-
rection is used by astronomers and navigators to establish a precise star transit time.

10.3  Debugging and Monitoring Commands

The DSP clock includes a primitive toolkit useful for debugging and evaluation. Debugging mode
can be turned on with one of the D commands and off with the D0 command. There are four

debug formats selected by the D1, D2, D3 and D4 commands, respectively. The output is inclu-

sive; that is, one, two or all three formats can be enabled at the same time, but all are disabled by

the D0 command.

D1

This command produces one line at second 59 of each minute in the same format as the U com-

mand described above.

D2

This command produces one line for each decoded timecode digit in the following format:

c m d n q sssss aaaaa mmmmm ddddd nnnnn eeeee

c clock digit_m maximum likelihood digit

d difference (mod 10) between clock and maximum likelihood digits

n compare counter (max 3)

q quality character_sssss 1-s sync epoch

aaaaa 1-s sync amplitude (threshold 1500)

mmmmm 1-m sync amplitude (threshold 500)

ddddd 100-Hz subcarrier amplitude (threshold 1000)

nnnnn noise estimate

eeeee digit correlator amplitude (threshold 1000)

D3

This command produces one line each second in the following format:

aaaaa eeeee ppppp fffff ccccc jjjjj vvvvv

aaaaa 1-s sync amplitude

eeeee median filter epoch of 1-s sync

ppppp median filter time offset

fffff time offset since last frequency update

ccccc compare counter (max 10)

jjjjj jitter counter (max equal to averaging cycle)

vvvvv averaging cycle counter

D4

This command produces one line at second 58 of each minute in the following format:

ddddd eeeee fffff ggggg hhhhh iiiii

ddddd DST1 integrator value

eeee DST2 integrator value

fffff leap warning integrator value

ggggg DUT± integrator value

hhhhh DUT1 integrator value

iiiii DUT2 integrator value

jjjjj DUT4 integrator value

10.4  Signal Generation and Monitoring

O{1-8}

This command selects certain signals to be monitoring in real time with an oscilloscope connected
to the DAC. The synthetic signals are synchronized with respect to the WWV/WWVH transmit-
ter, so may be useful as precision time and frequency sources for other devices, such as laboratory
test equipment. Note that the stuffing cycles necessary to produce the standard frequencies from
the DSP-93 hardware sample clock produce some phase modulation in the signals, which appear
as a low frequency buzz on the 1000/1200-Hz signal. The signals are selected with the O{1-8}
command, where the digit is:

1 input signal (after peak clipping, but before other processing)

2 output of 1-s sync comb filter_3 output of data bit matched filter

4 synthesized one-second ramp in 125-us increments

5 synthesized one-minute ramp in 1-s increments

6 synthesized 1000-Hz (WWV) or 1200-Hz (WWVH) sinewave

7 synthesized 100-Hz sinewave

8 data bit probability - positive (1), negative (0)

For the DC-coupled signals, the oscilloscope should be connected to JP210, pin 2; that is, the pin
closest to the power regulators. In the case of the ramps and bit probability, the lowpass filter in
the DSP-93 D/A limits the risetime and introduces a moderate degree of ringing.

A speaker can be connected to the DSP-93 output to monitor the operation of the program. The

O1 signal is useful for general watchkeeping. The O2 signal is probably the best indication that
the WWV/H signal is present. If a faint tick can be heard, the DSP clock can probably synchro-
nize to the signal. Normally, at the decision threshold where the tick can barely be heard, the

WWV/H signal cannot be heard in the unprocessed receiver output, although a faint beep may be
heard marking the first second of the minute. The O3 signal is best viewed with an oscilloscope,
where the waveform should appear as a trapezoid rising at the second and decaying either 200,

500 or 800 ms later. When viewed on an oscilloscope with a calibrated sweep delay and triggered
by a PPS signal from a source calibrated to UTC, the O4 signal becomes a precision proof-of-per-
formance indicator.

10.5  Operation Notes

The particular algorithms implemented in the DSP clock have not been thoroughly tested over
many months and seasons, nor have the various thresholds been experimentally verified under all
conditions. This applies especially to the decision thresholds, called bottom fishers, which deter-
mine whether a particular signal is usable or not. Since the DSP-93 program is designed to be very
aggressive in sifting signals from noise, if these thresholds are set too low, the program may
decode noise as UTC. On the other hand, if these thresholds are set too high, usable signals may
be ignored and the clock drift away from UTC. The current thresholds are defined in the output
formats described above and in the source code. They are probably set too low in an effort to
scrape the weakest signals from the noise. In normal operation, the values are several times the
thresholds.

There is a necessary design compromise between weak-signal sensitivity and DSP-93 clock oscil-

lator frequency tolerance. When first started, the program must discipline the sample clock to

within 12.5 PPM, in order to reliably identify the 1-s sync signal epoch. At the smallest averaging

interval (8 s) and largest jitter threshold (500
m
s) which can reliably extract the epoch, the toler-

ance must be less than 62.5 PPM. As the frequency offset of the DSP-93 used for program devel-

opment is over 45 PPM, this could be a problem in some units. While not tested, the program

should cope with tolerances greater than 62.5 PPM, but it will take significantly longer to syn-

chronize.

7.