16

PPS TC, IRIG

Timekeeping facilities at UDel - March 1996 l Cesium oscillator is calibrated by U.S. Naval Observatory and checked continuously by Northeast US LORAN-C chain and GPS l NTP primary time servers synchronize to timecode (TC), PPS and

IRIG-B, all with kernel modifications for precision timekeeping l NTP secondary servers (not shown) include VAX, SunOS 4/5, Ultrix 4,

OSF/1, HP-UX, Cisco, Bancomm and Fuzzball (semi-retired)

WWVB receivers (2)

GPS receivers (2)

Cesium oscillator

LORAN-C receivers (2)

WWv/B, CHU receivers (3) pogo

DCnet

rackety public

barnstable

DARTnet

UDELnet routers

grundoon

NTP monitor

TC, IRIG

PPS

DARTnet

1.5 Mb/s T1

UDELnet, NSFnet

1.5 Mb/s T1 (2)

DCnet 128.4

10/100 Mb/s

ISDN bridge